** **

**ABARTH TECHNICAL SPECIFICATIONS**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Engine | **Abarth 500** | **Abarth 500C** | | **Abarth Punto** |
| Layout | 4-Cyl in-line | | | 4-Cyl in-line MultiAir |
| Induction System | IHI Turbo, Fixed Geometry | | | Garrett GT1446 Turbo |
| Displacement (cc) | 1,368 | | | 1,368 |
| Power HP @RPM | 135 @ 5,500 | | | 163 @ 5,500 |
| Torque Nm @RPM | 206 @ 2,000 | | | 250 @ 2,500 |
| Transmission | 5-Speed Manual/FWD | | | 6-Sp Man/FWD |
| Steering Type | Rack and pinion with electric power steering with Sport Mode | | | |
| Brakes (F vented mm) | 284X22 54mm Floating Calliper | | 305X22 54mm Floating Calliper | |
| Brakes (R solid mm) | 240X11 34mm Floating Calliper | | 240X11 34mm Floating Calliper | |
| Front Suspension | McPherson strut, anti-roll bar | | | |
| Rear Suspension | Torsion beam, coil-over struts, anti-roll bar | | | |
| Dimensions (mm) | L3546 X W1672 X H1488 / WB2300 | | L4065 X W1721 X H1478 / WB2510 | |
| Boot Capacity (L) | 185 / 520 (seats folded) | | 275 / 1030 (seats folded) | |
| Tyres | Std: 205/40 R16 Opt: 215/45 R17 | | Std: 215/45 R17 Opt: 215/45 R17 | |
| Kerb weight (kg) | 1110 | 1150 | | 1260 |
| Fuel tank (litres) | 35 | 35 | | 37 |
| Max speed (km/h) | 205 | 205 | | 213 |
| 0–100 km/h | 7.9 | 7.9 | | 7.9 |
| L/100km (U/EU/C) | 8.5/5.4/6.5 | 8.5/5.4/6.5 | | 8.0/5.0/6.1 |
| CO2 (g/km) | 155 | 155 | | 142 |